{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作表1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作表1","index":0,"n_rows":26,"n_cols":19,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,0,0,19],[2,0,2,3],[2,4,2,19],[3,0,3,3],[3,4,3,9],[3,10,3,14],[3,15,3,19],[4,0,4,3],[4,4,4,9],[4,10,4,14],[4,15,4,19],[5,0,5,3],[5,4,5,19],[6,1,6,7],[6,8,6,17],[6,18,6,19],[7,2,7,7],[7,8,7,17],[8,2,8,7],[8,8,8,17],[9,2,9,7],[9,8,9,17],[10,2,10,7],[10,8,10,17],[11,2,11,7],[11,8,11,17],[12,2,12,7],[12,8,12,17],[13,5,13,6],[13,8,13,17],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,3,20,5],[20,6,20,9],[20,10,20,14],[20,15,20,19],[21,3,21,19],[22,3,22,15],[22,16,22,19],[24,3,24,4],[25,3,25,15],[25,16,25,19],[6,0,12,0],[13,0,19,0],[13,4,14,4],[15,5,19,5],[13,7,14,7],[7,18,12,19],[15,18,19,19],[13,18,14,19],[13,1,14,3],[23,0,25,2],[20,0,22,2]]}
["交通信号控制系统检验批质量验收记录"]
["质控（市政）表C.0.177"]
["单位工程名称",null,null,null,"顺义区2021年交通设施运行维护项目"]
["分部工程名称",null,null,null,"交通工程",{"$nulls":5},"验收部位",{"$nulls":4},"信号灯更换"]
["施工单位",null,null,null,"北京福通互联科技集团有限公司",{"$nulls":5},"项目经理"]
["施工执行标准名称及编号",null,null,null,"《道路交通信号灯按照规范》GB14886—2006；《交通信号灯》GB14887—2011；《道路交通智能管理系统设施设置规范》DB 12/596.1-2015；\r"]
["主控项目","施工质量验收规范的规定",{"$nulls":6},"施工单位检查评定记录",{"$nulls":9},"监理（建设）                     单位验收记录"]
[null,1,"预埋管道质量应符合设计及验收规范要求",{"$nulls":5},"合格",{"$nulls":9},"合格"]
[null,2,"控制电缆质量应符合设计及验收规范要求",{"$nulls":5},"合格"]
[null,3,"信号机品种及质量应符合设计及验收规范要求",{"$nulls":5},"合格"]
[null,4,"检查井质量应符合设计及验收规范要求",{"$nulls":5},"合格"]
[null,5,"基础混凝土强度应符合设计及验收规范要求",{"$nulls":5},"合格"]
[null,6]
["一般项目","序号项目",null,null,"允许偏差（mm）","检验频率",null,"检验方法","实测值或实测偏差值",{"$nulls":9},"监理（建设）                     单位验收记录"]
[{"$nulls":5},"范围（m）","点数",null,2,-2]
[null,1,"预埋管道埋设深度（mm）",null,"±5\r","每个信号灯",2,"用钢尺量",1,-1,{"$nulls":8},"合格"]
[null,2,"检查井安装深度（mm）",null,"±5\r",null,2,"用钢尺量",3,2]
[null,3,"立柱竖直度（mm）",null,"±3\r",null,2,"用21m小线和钢尺量",2,1]
[null,4,"金属构件镀层厚度（mm）",null,"标志柱、横梁≥78，紧固件≥50\r",null,2,"用垂线和钢尺量",14,2]
[null,5,"信号灯基础尺寸（mm）",null,"-50，+100",null,2,"用2m直尺、塞尺量",-8,57]
["施工单位     检验评定结果",null,null,"专业工长（施工员）",{"$nulls":6},"施工班组长"]
[null,null,null,"主控项目全部合格,一般项目满足规范规定要求。"]
[null,null,null,"项目专业质量检查员：",{"$nulls":12},"年    月    日"]
["监理（建设）单位验收结论"]
[null,null,null,"专业监理工程师："]
[null,null,null,"（建设单位项目专业技术负责人）",{"$nulls":12},"年    月    日"]