{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["环境设备","设备编号","环境设置","环境警报","监控数据展示"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"环境设备","index":0,"n_rows":11,"n_cols":12,"rows_kept":11,"cut":false,"hidden":false,"merged":[[10,0,13,11]]}
["设备编号","设备名称","设备类型","设备标识码","设备品牌","生产厂家","出厂日期","设备型号","安装日期","经度","纬度","设备状态"]
{"$rows_empty":9}
["设备类型：自动化、水肥一体化、农田环境、大棚环境\n出厂日期、安装日期：精确到日\n设备状态：启用、停用"]

{"sheet":"设备编号","index":1,"n_rows":9,"n_cols":7,"rows_kept":9,"cut":false,"hidden":false,"merged":[[8,0,10,6]]}
["隶属地块名称","设备编号","设备名称","地块类型","经度","纬度","设备状态"]
{"$rows_empty":7}
["这张表是设备与地块的对应关系表\n设备状态：取自环境设备的状态数据，环境设备停用，这边也会停用"]

{"sheet":"环境设置","index":2,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[[9,0,11,4]]}
["环境指标",null,null,null,"数据指标"]
["上限","上限持续时间（h）","下限","下限持续时间（h）","无数据持续时间"]
{"$rows_empty":7}
["上限、下限：保留3位小数\n上限持续时间（h）、下限持续时间（h）：整数"]

{"sheet":"环境警报","index":3,"n_rows":9,"n_cols":8,"rows_kept":9,"cut":false,"hidden":false,"merged":[[8,0,10,7]]}
["地块编号","地块名称","设备编号","设备名称","发生时间","警报值","持续时间（h）","警报类型"]
{"$rows_empty":7}
["发生时间：精确到时分秒\n警报类型：温度上限、温度下限、湿度上限、湿度下限、光照上限、光照下限、无数据警报、无图像警报\n警报值：保留3位小数\n警报：温度警报、湿度警报、光照警报持续一个小时及以上警报。\n无数据警报、无图像警报：持续24小时以上。"]

{"sheet":"监控数据展示","index":4,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[[11,0,13,7]]}
["隶属地块名称","设备编号","设备名称","空气温度（℃）","空气湿度（%）","光照（lux）","上报时间","图像查看"]
{"$rows_empty":10}
["上报时间：精确到时分秒\n图像查看：上报的图片。一般为2张。"]